**High\_level\_requirements:**

|  |  |  |
| --- | --- | --- |
| **ID** | **Description Category** | **status** |
| HR01 | Four rows must be printed | Implemented |
| HR02 | User must get the numbers printed in format given | Implemented |

**Low\_level\_requirements:**

|  |  |  |
| --- | --- | --- |
| **ID** | **Description Category** | **status** |
| LR01 | There should be a provision to enter the required number to be printed | Implemented |
| LR02 | Entered number should be converted to binary | Implemented |
| LR03 | The binary equivalent should be printed from LHS | Implemented |
| LR04 | The bits with binary ‘1’ should be printed as ‘\*’ | Implemented |
| LR05 | The bits with binary ‘0’ should be printed as ‘\_’ | Implemented |